1-download and install Arduino IDE

2-put the library in URL

3-from Board manager install esp32 "espressif system 1.0.06" and lick ok

4. Open the Boards Manager. Go to **Tools** , **Board** , **Boards Manager…**

5. go for **ESP32** and press install button for the **ESP32 by Espressif Systems**

6. and go to tool lick **DOIT ESP32 DEVKIT V1**

7- lick the buttom “ port (COM4)

8- open the ( file< Examples,Wifi<WifiScan)

9-and now create a new sketch

10-press the ( upload button < wait the code compiles <upload in the board )

11-see the (Done uploading Message)

12-open the ArduionIDE in baud

13. go the (ESP32)

14.Press the (115200baud)

15-press the (ENABLE)

16. Waite to run the new